<!--
title: "Adaptec RAID controller monitoring with Netdata"
custom_edit_url: https://github.com/netdata/netdata/edit/master/collectors/python.d.plugin/adaptec_raid/README.md
sidebar_label: "Adaptec RAID"
-->

# Adaptec RAID controller monitoring with Netdata

Collects logical and physical devices metrics.

## Requirements

The module uses `arcconf`, which can only be executed by root.  It uses
`sudo` and assumes that it is configured such that the `netdata` user can
execute `arcconf` as root without password.

Add to `sudoers`:

```
netdata ALL=(root)       NOPASSWD: /path/to/arcconf
```

To grab stats it executes:

-   `sudo -n arcconf GETCONFIG 1 LD`
-   `sudo -n arcconf GETCONFIG 1 PD`

It produces:

1.  **Logical Device Status**

2.  **Physical Device State**

3.  **Physical Device S.M.A.R.T warnings**

4.  **Physical Device Temperature**

## Configuration

**adaptec_raid** is disabled by default. Should be explicitly enabled in `python.d.conf`.

```yaml
adaptec_raid: yes
```

Edit the `python.d/adaptec_raid.conf` configuration file using `edit-config` from the Netdata [config
directory](/docs/configure/nodes.md), which is typically at `/etc/netdata`.

```bash
cd /etc/netdata   # Replace this path with your Netdata config directory, if different
sudo ./edit-config python.d/adaptec_raid.conf
```



![image](https://user-images.githubusercontent.com/22274335/47278133-6d306680-d601-11e8-87c2-cc9c0f42d686.png)

---

[![analytics](https://www.google-analytics.com/collect?v=1&aip=1&t=pageview&_s=1&ds=github&dr=https%3A%2F%2Fgithub.com%2Fnetdata%2Fnetdata&dl=https%3A%2F%2Fmy-netdata.io%2Fgithub%2Fcollectors%2Fpython.d.plugin%2Fadaptec_raid%2FREADME&_u=MAC~&cid=5792dfd7-8dc4-476b-af31-da2fdb9f93d2&tid=UA-64295674-3)](<>)
