SiteMap ENGLISH 中文站

- LED Downlight

- 1*1W
- 3*1W
- 5*1W
- 6*1W
- 7*1W
- 9*1W
- 12*1W

- LED Tube Light

- LED T5 Tube Light
- LED T8 Tube Light
- LED T10 Tube Light

- LED Ceiling Light

- 1*3W
- 3*1W
- 9*1W
- 18*1W
- 27*1W
- 36*1W

- LED Panel Light

- LED Spot Light

- 1*3W
- 3*1W
- 3*2W
- 4*1W
- 5*1W
- 6*1W
- 7*1W
- 9*1W
- 12*1W

- LED Bulb Light

- 1*3W
- 1*5W
- 3*1W
- 4*1W
- 5*1W
- 6W
- 7*1W
- 9*1W

- LED Candle Light

- 1*3W
- 3*1W

Led products
Home / Led products/LED Panel Light
Model:LED Panel Light-OKT-PL-16-L6W3

LED Quantity: | 240pcs
LED Type: | SMD3528
Luminous Flux: | 1320lm
Beam Angle: | 120°
Power Consumption: | 16W
Input Voltage: | AC85-265V

Download:

PARAMETERS | BENEFIT | APPLICATION | INQUIRY NOW

Parameter | Value
LED Type: | High Quality SMD3528
LED Quantity: | 240pcs
Power Consumption: | 16W
Input Voltage: | AC85-265V
Operating Current: | 20 mA
IP Code: | IP50 / Class Ⅲ
Color Temperature: | Warm white(2700-3500K); Neutral white(3800-4800K); Cool white(5500-6500K)
Luminous Flux: | 1320lm
Color Rendering Index: | Ra≥80
Beam Angle: | 120°
Weight: | 2.6KG
Base Type: |
Housing Material & Color: | Aluminum alloy and Acrylic cover; Silver
LED Rated Life: | 50,000 hours
Opetating Temperature: | -20 ~ +50
Storage Temperature: | -20 ~ +80
Dimension(mm): | 300*600*15
Dimmability: | Available
Certification: | CE & ROHS
1. Special optical design of the transparent diffusers, the original concentrate light from LED is transmitted into uniform illuminance. Since the lamp chimneys apply the pure optical diffuser design, the light transmittance rate is high, and it also solves the LED lighting problems of transmittance, glare and diffuser. 2. Import super light poscap LED light source, which has a long working life and consume less power (save more than 90% energy than incandescent light, and 60% than fluorescent light). 3. It is no hazardous material such as lead and mercury. The products are green and environmental friendly. No heat radiation and ultraviolet rays from the light protect your health. 4. The color index of the light source makes the color of office equipments look better. 5. To start, no stroboflash and less asthenopia.
This product Used in Office areas, factory, shopping malls, subways and washrooms.
Advisory products: | *
Company: |
Your name: | *
Tel: | *
Fax: |
Email: | *
Address: |
Your advice: | *
Check Code: |

PREV:1*1W LED Downlight OKT-DL-1A1-SA
NEXT:LED Panel Light-OKT-PL-14-R240