SiteMap ENGLISH 中文站

- LED Downlight

- 1*1W
- 3*1W
- 5*1W
- 6*1W
- 7*1W
- 9*1W
- 12*1W

- LED Tube Light

- LED T5 Tube Light
- LED T8 Tube Light
- LED T10 Tube Light

- LED Ceiling Light

- 1*3W
- 3*1W
- 9*1W
- 18*1W
- 27*1W
- 36*1W

- LED Panel Light

- LED Spot Light

- 1*3W
- 3*1W
- 3*2W
- 4*1W
- 5*1W
- 6*1W
- 7*1W
- 9*1W
- 12*1W

- LED Bulb Light

- 1*3W
- 1*5W
- 3*1W
- 4*1W
- 5*1W
- 6W
- 7*1W
- 9*1W

- LED Candle Light

- 1*3W
- 3*1W

Led products
Home / Led products/LED Spot Light
Model:3*1W LED Spot Light-OKT-SL-3B1-E27

LED Quantity: | 3PCS
LED Type: | CREE/EPISTAR
Luminous Flux: | Cool white 285lm; Warm white 264lm
Beam Angle: | 38°/60°
Power Consumption: | 4W
Input Voltage: | AC85-265V

Download:

PARAMETERS | BENEFIT | APPLICATION | INQUIRY NOW

Parameter | Value
LED Type: | CREE/EPISTAR
LED Quantity: | 3PCS
Power Consumption: | 4W
Input Voltage: | AC85-265V
Operating Current: | 330±10mA
IP Code: | IP60 / Class
Color Temperature: | Warm white(2700-3500K); Neutral white(3800-4800K); Cool white(5500-6500K)
Luminous Flux: | Cool white 285lm; Warm white 264lm
Color Rendering Index: | Ra≥80
Beam Angle: | 38°/60°
Light Distribution: | Clear, Faceted , Frosted Lens
Base Type: | GU10 / E27 / MR16 for options
Housing Material & Color: | Aluminum alloy & Silver
LED Rated Life: | 50,000 hours
Operating Temperature: | -20 ~ +50
Storage Temperature: | -20 ~ +80
Dimension:(mm) | H69.51*D50
Dimmability: | N/A
Weight: | 56.6g
Certification: | CE & ROHS
1. Adopting high brightness and small light decline for leds; 2. Adopting excellent aluminum alloy heat dissipation structure; 3. Longer life with high efficiency constant current driver,more than 50,000 hours; 4. No noise, non-UV, infrared radiation, no strobe light, quick response and protect eyes,to ensure that the use of the comfortable and health; 5. High efficiency and energy saving, only 25-50% power consumption compare with traditional lamp; 6. No mercury / lead / halogen powder hazardous substances; 7. No maintenance cost.
1.Supermarket/showcase/shopwindow; 2.Museum/exhibition room; 3.Coffee house/bar/ western restaurants; 4.Others(the place where need spot lighting).
Advisory products: | *
Company: |
Your name: | *
Tel: | *
Fax: |
Email: | *
Address: |
Your advice: | *
Check Code: |

PREV:1*1W LED Downlight OKT-DL-1A1-SA
NEXT:3*1W LED Spot Light-OKT-SL-3D1-MR16